• Single phase model used to simulate the nanofluids flow inside microchannel.

• Effects of using LVGs and nanofluids on convectional heat transfer coefficient has been investigated.

• Variations of heat transfer coefficient and Nusselt number reported for different Reynolds number and nanoparticle volume concentrations.